**CFM01.02 - Components: design of components leads to mismatch errors during maintenance**

Component sets can be separated. Mismatched components are used in error, resulting in a high pressure wheel assembly failure.

Credible Failure mode is addressed by:

View in tabBI.02.10 Wheel assembly component register

View in tabBI.02.11 Wheel assembly component inspection before first use or re use

View in tabBI.02.12 Wheel and rim components are clearly identified by the OEM

View in tabBI.02.13 Wheel and rim OEM provide catalogues of their products and advice on use

View in tabBI.02.21 Error tolerant design of wheel assembly components